{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":12,"rows_kept":41,"flags":["formulas_cached_only"]}
["类型编号","试题类型","试题编号","题型(单选题、多选题、判断题)","适合岗位","试题内容","答案项A","答案项B","答案项C","答案项D","答案项E","正确答案项"]
[{"v":1,"d":"001"},"入场培训试题","00001","单选题","起重吊装工","起重机械的信号员的主要责任是（   ）","考核起重机操作员的工作表现","在吊运过程中，给操作员适当的指示信号，令吊运工作顺利进行","负责维修起重机的信号系统",null,null,"C"]
[{"v":2,"d":"002"},"入场培训试题","00002","单选题","起重吊装工","对吊装施工最有指导意义的是(    )","起重施工方案","设备平面布置图","流程图",null,null,"A"]
[{"v":3,"d":"003"},"入场培训试题","00003","单选题","起重吊装工","履带式吊车上下坡时悬臂的放置方位是(  )","上坡时朝前方下坡时朝后方","上坡时朝后方下坡时朝前方","上下坡都朝前方",null,null,"C"]
[{"v":4,"d":"004"},"入场培训试题","00004","单选题","起重吊装工","选用2台千斤顶起重时每台千斤顶的起重量不应小于计算载荷是倍数(   )","3倍","1.2倍","0.8倍",null,null," B"]
[{"v":5,"d":"005"},"入场培训试题","00005","单选题","起重吊装工","起重机接近终点时，应该(   )","及时断电，尽可能不动用行程限位器","等待行程限位器动作","加快起重机动作速度",null,null,"A"]
[{"v":6,"d":"006"},"入场培训试题","00006","单选题","起重吊装工","钢丝绳在使用过程中应经常检查其强度，一般每（  ）个月检查一次",5,6,7,8,null,"B"]
[{"v":7,"d":"007"},"入场培训试题","00007","单选题","起重吊装工","钢丝绳径向磨损或腐蚀量超过原直径的（   ）应报废",0.3,0.4,0.45,0.5,null,"B"]
[{"v":8,"d":"008"},"入场培训试题","00008","单选题","起重吊装工","吊钩危险断面磨损达原尺寸的（  ）时应报废",0.04,0.08,0.1,0.15,null,"C"]
[{"v":9,"d":"009"},"入场培训试题","00009","单选题","起重吊装工","绳夹安全使用要求：每个绳夹均应拧紧，以压扁钢丝绳直径(  ）为宜","1/2","1/3","1/4","1/5",null,"B"]
[{"v":10,"d":"010"},"入场培训试题","00010","单选题","起重吊装工","指挥物体翻转时，应使其重心（  ），不应产生指挥意图之外的动作","失稳变化","平稳变化","平稳快速变化","随意变化",null,"B"]
[{"v":11,"d":"011"},"入场培训试题","00011","单选题","起重吊装工","三宝指（  ）","安全帽、安全带、安安全帽、绝缘手套、防护面罩全网",null,"绝缘手套、安全网、安全绳","安全网、安全锁、安全绳",null,"A"]
[{"v":12,"d":"012"},"入场培训试题","00012","单选题","起重吊装工","安全是（   ）","没有危险的状态","没有事故的状态","舒适的状态","生产系统中人员免遭不可承受危险的伤害",null,"D"]
[{"v":13,"d":"013"},"入场培训试题","00013","单选题","起重吊装工","根据《安全色》规定，安全色分为红、黄、蓝、绿四种颜色，分别表示（   ）","禁止、指令、警告和提示","指令、禁止、警告和提示","禁止、警告、指令和提示","提示、禁止、警告和指令",null,"C"]
[{"v":14,"d":"014"},"入场培训试题","00014","单选题","起重吊装工","下列关于安全标志含义的叙述，不正确的是（ ）","禁止标志，含义是不准或制止人们某种行为","警告标志，含义是警告人们当心、小心、注意","指令标志，含义是必须遵守","提示标志，含义是提示人们不能去做",null,"D"]
[{"v":15,"d":"015"},"入场培训试题","00015","单选题","起重吊装工","《安全生产法》规定，特种作业人员必须经专门的安全作业培训。取得特种作业（  ）证书，方可上岗作业","操作资格","许可","安全","岗位",null," A"]
[{"v":16,"d":"016"},"入场培训试题","00016","单选题","起重吊装工","依照《安全生产法》规定，生产经营单位必须保证上岗的从业人员都经过（  ），否则，生产经营单位要承担法律责任","安全生产教育","安全技术培训","安全作业培训","安全生产教育和培训",null,"D "]
[{"v":17,"d":"017"},"入场培训试题","00017","单选题","起重吊装工","遇有（ ）以上强风、浓雾等恶劣气候，不得进行露天攀登与悬空高处作业","5级","6级","7级   ","8级",null,"B "]
[{"v":18,"d":"018"},"入场培训试题","00018","单选题","起重吊装工","在起重作业中，（  ）斜拉、斜吊和起吊地下埋设或凝结在地面上的重物","允许","禁止","应设专人监控","采取措施后可以",null,"B"]
[{"v":19,"d":"019"},"入场培训试题","00019","单选题","起重吊装工","起重机械超载限制器在载荷达到（）时应能发出警示性信号",0.7,0.8,0.9,0.95,null,"C"]
[{"v":20,"d":"020"},"入场培训试题","00020","单选题","起重吊装工","高处作业的下列几项安全措施中，哪一项是首先需要的?","安全带","安全网","合格的工作台",null,null,"C"]
[{"v":21,"d":"021"},"入场培训试题","00021","判断题","起重吊装工","凡离地面2米以上的地点进行工作，都应视作高处作业，在1.5米高处没有栏杆的脚手架上作业可以不系安全带","正确","错误",{"$nulls":3},"B"]
[{"v":22,"d":"022"},"入场培训试题","00022","判断题","起重吊装工","高处作业应一律使用工具袋，较大的工具应用绳栓在牢固的构件上。禁止挂在移动或不牢固的物件上","正确","错误",{"$nulls":3},"A"]
[{"v":23,"d":"023"},"入场培训试题","00023","判断题","起重吊装工","15米以上高处作业必须办理许可手续","正确","错误",{"$nulls":3},"A"]
[{"v":24,"d":"024"},"入场培训试题","00024","判断题","起重吊装工","安全带要拴挂在牢固的构件或物体上，要防止摆动或碰撞，绳子不能打结使用， 钩子要挂在连接环上","正确","错误",{"$nulls":3},"A"]
[{"v":25,"d":"025"},"入场培训试题","00025","判断题","起重吊装工","四级风力及其以上应停止一切吊运作业","正确","错误",{"$nulls":3},"B"]
[{"v":26,"d":"026"},"入场培训试题","00026","判断题","起重吊装工","吊钩由于长期使用产生剥裂，必须对其焊接修补后方可继续使用","正确","错误",{"$nulls":3},"B"]
[{"v":27,"d":"027"},"入场培训试题","00027","判断题","起重吊装工","司机对任何人发出的紧急停止信号，均应服从","正确","错误",{"$nulls":3},"A"]
[{"v":28,"d":"028"},"入场培训试题","00028","判断题","起重吊装工","卷扬机安装位置应选择视野宽阔的地方，便于卷扬机司机和指挥人员观察","正确","错误",{"$nulls":3},"A"]
[{"v":29,"d":"029"},"入场培训试题","00029","判断题","起重吊装工","起重机工作时的停放位置应与沟渠、基坑保持安全距离。且作业时不得停放在 斜坡上 进行","正确","错误",{"$nulls":3},"A"]
[{"v":30,"d":"030"},"入场培训试题","00030","判断题","起重吊装工","作业前应将支腿全部伸出，并支垫牢固。调整支腿应在无 载荷 时进行，并将起重臂全部缩回转至 正前或正后 ，方可调整。作业过程中发现支腿沉陷或其它不正常情况时，应立即放下 吊物 ，进行调整后，方可继续作业。","正确","错误",{"$nulls":3},"A"]
[{"v":31,"d":"031"},"入场培训试题","00031","多选题","起重吊装工","从业人员可以行使（    ）权利","从业人员有权对本单位安全生产工作中存在的问题提出批评、检举、控告","有权拒绝违章指挥和强令冒险作业","从业人员有权了解其作业场所和工作岗位存在的危险因素、防范措施及事故应急措施","对本单位的安全生产工作提出建议",null,"A,B,C,D"]
[{"v":32,"d":"032"},"入场培训试题","00032","多选题","起重吊装工","起重吊装前指挥人员需确认（   ）","确认危险区域无人","确认吊车吊件安全","确认吊具吊点正确","确认人员经过培训","确认引绳准备到位","A,B,C,D"]
[{"v":33,"d":"033"},"入场培训试题","00033","多选题","起重吊装工","“四不伤害”是广大劳动群众在实践中总结出来的安全事故预防原则，其内容为（  ）","不伤害自己","不伤害他人","保护他人不受伤害","不被他人伤害",null,"A,B,C,D"]
[{"v":34,"d":"034"},"入场培训试题","00034","多选题","起重吊装工","以下哪些人不许参加高处作业（    ）","高血压人员，心脏病人员","施工人员","技术人员","癫痫病人",null,"A,D"]
[{"v":35,"d":"035"},"入场培训试题","00035","多选题","起重吊装工","吊车卷扬注意事项包括（  ）","货物起吊的过程中起重机每转换一次动作应鸣笛","吊钩处于最低位置时，卷筒上的钢丝绳不得少于3圈","纲丝绳直径与卷筒上的绳槽直径相匹配","钢丝绳插头不规范过短",null,"A,B,C"]
[{"v":36,"d":"036"},"入场培训试题","00036","多选题","起重吊装工","起重机械常见安全隐患包括（  ）","未安装荷载限制装置未安装行程限位装置或不灵敏或不灵敏",null,"起重拔杆组装不符合设计要求","起重拔杆组装后未履行验收程序或验收表无责任人签字",null,"A,B,C,D"]
[{"v":37,"d":"037"},"入场培训试题","00037","多选题","起重吊装工","索具常见安全隐患包括（   ）","索具采用编结连接时，编结部分的长度不符合规范要求","索具采用绳夹连接时，绳夹的规格、数量及绳夹间距不符合规范要求","索具安全系数不符合规范要求","吊索规格不匹配或机械性能不符合设计要求",null,"A,B,C,D"]
[{"v":38,"d":"038"},"入场培训试题","00038","多选题","起重吊装工","为保证履带式起重机的安全使用，必须做到（ ）","禁止斜拉","严禁起吊埋设在地下的重物","严禁起吊凝结在地面上的重物","路基的承载力足够",null,"A,B,C,D"]
[{"v":39,"d":"039"},"入场培训试题","00039","多选题","起重吊装工","起重机的基本结构包括（  ）","起升机构","运行机构","旋转机构","电气系统",null,"A,B,C,D"]
[{"v":40,"d":"040"},"入场培训试题","00040","多选题","起重吊装工","钢丝绳的捻绕方式包括（  ）","同向捻","交互捻","混合捻","反向捻",null,"A,B,C"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}