{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["日常检查表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"日常检查表","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[0,0,0,5],[1,1,1,2],[2,1,7,1],[4,2,5,2],[9,1,10,1],[9,2,10,2],[11,1,14,1],[13,2,14,2],[16,1,17,1],[18,0,19,0],[18,1,19,5],[20,0,21,0],[20,1,20,5],[21,1,21,5]],"flags":["formulas_cached_only"]}
["起重机械（塔吊）日常检查表"]
["序号","项目",null,"检查方法、内容及要求","是否符合要求","备注"]
[1,"整机","安全距离","目测塔机与相邻塔机、障碍物、架空输电线等安全距离符合GB5144的规定"]
[2,null,"压重","目测固定可靠，无移位"]
[3,null,"基础","目测（必要时使用扳手）检查底部、塔身撑杆固定可靠无松动"]
[4,null,null,"目测基础无积水无异常变动"]
[5,null,"螺栓连接","目测各连接螺栓已按说明书要求拧紧、锁定无松动"]
[6,null,"现场整理","塔机上无可能坠落的杂物"]
[7,"结构","附着","目测结构无变动、连接紧固无松动"]
[8,"机构","起升、变幅、回转、运行机构","空运转无异常噪声、制动动作可靠"]
[9,null,null,"抗风防滑装置无缺损、无可见裂纹"]
[10,"关键零部件","吊钩","目测防脱钩装置完整有效"]
[11,null,"钢丝绳","目测钢丝绳未脱股、断丝等达到报废"]
[12,null,"滑轮与卷筒","目测钢丝绳防脱槽装置完好"]
[13,null,null,"滑轮运转灵活，轮缘无破损"]
[14,"电控系统","配电箱","塔吊专用，严禁接入其他"]
[15,"安全防护","行程限制器","空载运行试验幅度、高度、行走及回转限位动作灵敏有效"]
[16,null,"标志与标牌","目测塔机标识标牌清晰，无缺失"]
["检查结论"]
[]
["检查人员签字","                                                                                                                                                                                                                                                                                                                                                                                                                           "]