{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":2,"n_cols":23,"rows_kept":2,"flags":["formulas_cached_only"]}
["单位编号","单元号\nArea code","试压包","管线号Line NO.1","管线号Line NO2.","流体代号Fluid Code","管道等级Piping Class","设计压力DES. Mpa(G)","设计温度DES.T(℃)","操作压力OPER. Mpa(G)","操作温度\nOPER. T(℃)","试验介质Test Medium","试验压力Test Mpa(G)","压管级别Piping Grade","P&ID NO.","抽检代号NDE Code","尺寸","管径","起点","终点","泄露试验压力","吹洗方式","REMARK"]
["14HJ","511","32001-CWR-001","TK51101","CWR-010001","CWR2","A1B","0.7","60","0.25","41.5","CWR2","1.05","","P07-11/14","","40","1000.0","盲法兰","地下管网","","人工清理"]